Generic 7.60
Replaces 1156, 1428, 1456 for CD112A

Packaged build | 010914b-1461C-ATI
Request number | 1461
Submitter | Jcrespi

Base build | 010914b
Platform | Rage 6
Stream | Base
Release | 7.60
OS | Win9x WinNT Win2k WinXP
Package | Standard Image
Languages | ENU JPN ARA CHS CHT CSY DAN DEU ELL ESP FIN FRA HEB HUN ITA KOR NLD NOR PLK PTB RUS SVE THA TRK

Program | DID | VID | SS ID | SSV ID
G-84802-R200-AiW 64MB DDR PAL | 4242 | 1002 | 02AA | 1002
H-76803-Radeon-32MB SDR VGA 160 | 5144 | 1002 | 0008 | 1002
H-75703-Radeon-32MB SDR VGA 200 | 5144 | 1002 | 0009 | 1002
H-70701-Radeon-64MB DDR VGA 166 | 5144 | 1002 | 000A | 1002
G-70703-Radeon-64MB DDR VIVO 183 | 5144 | 1002 | 001A | 1002
G-76701-Radeon-AiW Radeon SDR PCI | 5144 | 1002 | 0029 | 1002
H-76809-Radeon-32MB SDR VGA VO 160 NTSC | 5144 | 1002 | 0038 | 1002
H-83801-Radeon-64MB SDR VGA VO | 5144 | 1002 | 0038 | 1002
G-75704-Radeon-32MB SDR VGA VO 166 NTSC | 5144 | 1002 | 0039 | 1002
G-70603-Radeon-32MB DDR VGA 166 | 5144 | 1002 | 008A | 1002
H-74903-Radeon-32MB DDR VGA VO 166 | 5144 | 1002 | 00BA | 1002
H-75702-Radeon-32MB SDR VGA DVI VO 166 NTSC | 5144 | 1002 | 0139 | 1002
H-76201-Radeon-32MB DDR DVI 166 Low Profile | 5144 | 1002 | 028A | 1002
G-73701-Radeon-AiW Radeon DDR AGP | 5144 | 1002 | 02AA | 1002
H-77801-Radeon-64MB DDR VGA DVI VO 200 | 5144 | 1002 | 053A | 1002
G-85707-R200-64MB DDR VGA2 DVI-I VO | 514C | 1002 | 013A | 1002
G-83202-RV200 64MB DDR VGA DVI-I VO | 5157 | 1002 | 013A | 1002
G-78507-RadeonVE-32MB DDR VGA DH | 5159 | 1002 | 000A | 1002
H-82102-RadeonVE 32MB SDR VGA VO DH ATX | 5159 | 1002 | 0038 | 1002
G-78512-RadeonVE-32MB DDR VGA VO DH | 5159 | 1002 | 003A | 1002
H-80004-RadeonVE-32MB DDR VGA VO DH LP | 5159 | 1002 | 00BA | 1002
G-78502-RadeonVE-32MB DDR VGA DVI-I VO DH | 5159 | 1002 | 013A | 1002

Feature | Option (* - override) | OS | Details
Mobile 440BX Chipset Support | Disable | Win9x | View details
Desktop | Icon and help screen | All | View details
Desktop Brightness | No Change | All | View details
Uninstall | Clean | All | View details
WDM drivers | Enable | All | View details
Multimedia Library | Enable | All | View details
Change Capture field Mode | No Change | All | View details
'DisableVPE' flag | Enable | All | View details
ATI Legacy Macrovision Support | Enable | All | View details
'DisableLCD' flag | Enable | All | View details
Problem Report | Enable | All | View details
InstallShield options | Normal install | All | View details
DAL Resume Support | Disable | All | View details
Details and diagnostic pages | Enable | All | View details
Use C3 Extended HotKey Polling Interval | Disable | Win2K | View details
Disable DAL check of Max Horizontal Frequency Range | Enable | Win2K | View details
OpenGL | Enable (7.57C and up) | All | View details
Hot-plug poller | Disable R6 (Enable Mobile) | All | View details
Tiling Support | Enable Tiling support | All | View details
Desktop Panning | Disable | All | View details
DAL flags | R6 Generic | All | View details
TVOut Filters | Normal | All | View details
Default mode | 640x480x8 | Win9x | View details
DPMS Screen Saver | Enable | WinNT | View details
Win2K 'Disable multimonitor' flag | Do not add key | All | View details
Projector Page | Disable the Projector Page | All | View details
DirectX Detection | Normal-No Change | All | View details
'DisableTimeStampWriteBack' flag | Enable | WinXP | View details
Images on the Displays Page | Normal | All | View details
Use Driver to detect EDID | Enable | Win9x | View details
'ExcludeFromSelect=*' entry | Enable | WinXP | View details
Win9x DVD support | Enable | Win9x | View details
DisableDrawPath | Normal | Win2K | View details
OpenGL "shared back/z" | Normal (Disabled) | All | View details
DriverInfoAddreg | Enabled | All | View details
Dual View | Enable | All | View details
Htime calculation logic in DAL | Enabled | Win9x | View details
ATI DDC2C support | Disable | All | View details
Anti-Alias | Application Preference | All | View details
Propagate VGA Expansion Setting in BIOS to Accelerated Drivers | Disable | All | View details
Default Z-Buffer setting | 16, 24 - 8-bit stencil | All | View details
Non-DDC CRT Support | Disabled | Win2K | View details
Extend Desktop | Normal | Win9x | View details
Brightness Mapping | Disable | All | View details
Force D3D driver to allocate vertex buffer | AGP memory | Win2K | View details
Disable AGP | Disable | All | View details

Signability test results (for information purposes only):

Win 2K Passed

Win 9X Passed

Win NT Passed

Win XP Passed

System version 1.86